# Example hostapd build time configuration
#
# This file lists the configuration options that are used when building the
# hostapd binary. All lines starting with # are ignored. Configuration option
# lines must be commented out complete, if they are not to be included, i.e.,
# just setting VARIABLE=n is not disabling that variable.
#
# This file is included in Makefile, so variables like CFLAGS and LIBS can also
# be modified from here. In most cass, these lines should use += in order not
# to override previous values of the variables.

# Driver interface for Host AP driver
CONFIG_DRIVER_HOSTAP=y

# Driver interface for wired authenticator
CONFIG_DRIVER_WIRED=y

# Driver interface for Prism54 driver
CONFIG_DRIVER_PRISM54=y

# IEEE 802.11F/IAPP
CONFIG_IAPP=y

# WPA2/IEEE 802.11i RSN pre-authentication
CONFIG_RSN_PREAUTH=y

# PeerKey handshake for Station to Station Link (IEEE 802.11e DLS)
CONFIG_PEERKEY=y

# IEEE 802.11w (management frame protection)
# This version is an experimental implementation based on IEEE 802.11w/D1.0
# draft and is subject to change since the standard has not yet been finalized.
# Driver support is also needed for IEEE 802.11w.
CONFIG_IEEE80211W=y

# Integrated EAP server
CONFIG_EAP=y

# EAP-MD5 for the integrated EAP server
CONFIG_EAP_MD5=y

# EAP-TLS for the integrated EAP server
CONFIG_EAP_TLS=y

# EAP-MSCHAPv2 for the integrated EAP server
CONFIG_EAP_MSCHAPV2=y

# EAP-PEAP for the integrated EAP server
CONFIG_EAP_PEAP=y

# EAP-GTC for the integrated EAP server
CONFIG_EAP_GTC=y

# EAP-TTLS for the integrated EAP server
CONFIG_EAP_TTLS=y

# EAP-SIM for the integrated EAP server
CONFIG_EAP_SIM=y

# EAP-AKA for the integrated EAP server
CONFIG_EAP_AKA=y

# EAP-PAX for the integrated EAP server
CONFIG_EAP_PAX=y

# EAP-PSK for the integrated EAP server (this is _not_ needed for WPA-PSK)
CONFIG_EAP_PSK=y

# EAP-SAKE for the integrated EAP server
CONFIG_EAP_SAKE=y

# EAP-GPSK for the integrated EAP server
CONFIG_EAP_GPSK=y
# Include support for optional SHA256 cipher suite in EAP-GPSK
CONFIG_EAP_GPSK_SHA256=y

# PKCS#12 (PFX) support (used to read private key and certificate file from
# a file that usually has extension .p12 or .pfx)
CONFIG_PKCS12=y

# RADIUS authentication server. This provides access to the integrated EAP
# server from external hosts using RADIUS.
CONFIG_RADIUS_SERVER=y

# Build IPv6 support for RADIUS operations
CONFIG_IPV6=y

CONFIG_DRIVER_NL80211=y

CONFIG_IEEE80211N=y

CONFIG_LIBNL32=y

CONFIG_ACS=y
