Description: Do not use /var/run
Author: Mathieu Malaterre <malat@debian.org>
Origin: vendor
Forwarded: not-needed

--- pbbuttonsd-0.8.1a.orig/pbbuttonsd.1
+++ pbbuttonsd-0.8.1a/pbbuttonsd.1
@@ -530,7 +530,7 @@ after connecting new input devices. Scan
 signal to the server:
 .PP
 .ad c
-kill \-HUP \`cat /var/run/pbbuttonsd.pid\`
+kill \-HUP \`cat /run/pbbuttonsd.pid\`
 .PP
 .ad b
 Be aware that the configuration file will also be reloaded in this case.
--- pbbuttonsd-0.8.1a.orig/src/init.h
+++ pbbuttonsd-0.8.1a/src/init.h
@@ -23,7 +23,7 @@
 #define ARG_QUIET		'q'
 
 #define DEFAULT_CONFIG	SYS_CONF_DIR "/pbbuttonsd.cnf"
-#define DEFAULT_PIDFILE "/var/run/" PACKAGE ".pid"
+#define DEFAULT_PIDFILE "/run/" PACKAGE ".pid"
 #define MODULECOUNT   15
 
 /**
--- pbbuttonsd-0.8.1a.orig/src/module_acpi.h
+++ pbbuttonsd-0.8.1a/src/module_acpi.h
@@ -21,7 +21,7 @@
 #  define PATH_ACPI		"/proc/acpi"
 #endif
 
-#define ACPID_SOCKET	"/var/run/acpid.socket"
+#define ACPID_SOCKET	"/run/acpid.socket"
 
 /**
  * @brief  Battery data
