# Template file for 'cubietruck-base'
pkgname=cubietruck-base
version=2.3
revision=2
build_style=meta
homepage="http://www.voidlinux.org"
short_desc="Void Linux Cubietruck (Cubieboard 3) platform package"
maintainer="Orphaned <orphan@voidlinux.org>"
license="Public Domain"

archs="armv7l"
depends="virtual?ntp-daemon cubietruck-uboot sun7i-kernel linux-firmware-network"

do_install() {
	# Load the sunxi-emac module by default.
	vmkdir usr/lib/modules-load.d
	echo sunxi-emac > ${DESTDIR}/usr/lib/modules-load.d/cubietruck.conf
	# Set proper perms to some devices.
	vmkdir usr/lib/udev/rules.d
	echo 'KERNEL=="disp|cedar_dev|mali|ump", MODE="0660", GROUP="video"' > ${DESTDIR}/usr/lib/udev/rules.d/50-cubietruck.rules
}
